# TMS430 Programming Notes

Always at the beginning of a program:

WDTCTL = WDTPW | WDTHOLD;

Stops the watchdog

Buttons on Launchpad => Connected directly to pin (no resistance neither condenser)

5 Lug 2020

CodeComposerStudio works fine but Enengia doesn’t